/* Definitions of prototypes for MIPS built-in functions.  -*- C -*-
   Copyright (C) 2007-2016 Free Software Foundation, Inc.

This file is part of GCC.

GCC is free software; you can redistribute it and/or modify
it under the terms of the GNU General Public License as published by
the Free Software Foundation; either version 3, or (at your option)
any later version.

GCC is distributed in the hope that it will be useful,
but WITHOUT ANY WARRANTY; without even the implied warranty of
MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
GNU General Public License for more details.

You should have received a copy of the GNU General Public License
along with GCC; see the file COPYING3.  If not see
<http://www.gnu.org/licenses/>.  */

/* Invoke DEF_MIPS_FTYPE (NARGS, LIST) for each prototype used by
   MIPS built-in functions, where:

      NARGS is the number of arguments.
      LIST contains the return-type code followed by the codes for each
        argument type.

   Argument- and return-type codes are either modes or one of the following:

      VOID for void_type_node
      INT for integer_type_node
      POINTER for ptr_type_node

   (we don't use PTR because that's a ANSI-compatibillity macro).

   Please keep this list lexicographically sorted by the LIST argument.  */
DEF_MIPS_FTYPE (1, (DF, DF))
DEF_MIPS_FTYPE (2, (DF, DF, DF))

DEF_MIPS_FTYPE (2, (DI, DI, DI))
DEF_MIPS_FTYPE (2, (DI, DI, SI))
DEF_MIPS_FTYPE (3, (DI, DI, SI, SI))
DEF_MIPS_FTYPE (3, (DI, DI, USI, USI))
DEF_MIPS_FTYPE (3, (DI, DI, V2HI, V2HI))
DEF_MIPS_FTYPE (3, (DI, DI, V4QI, V4QI))
DEF_MIPS_FTYPE (2, (DI, POINTER, SI))
DEF_MIPS_FTYPE (2, (DI, SI, SI))
DEF_MIPS_FTYPE (2, (DI, USI, USI))

DEF_MIPS_FTYPE (2, (INT, DF, DF))
DEF_MIPS_FTYPE (2, (INT, SF, SF))
DEF_MIPS_FTYPE (2, (INT, V2SF, V2SF))
DEF_MIPS_FTYPE (4, (INT, V2SF, V2SF, V2SF, V2SF))

DEF_MIPS_FTYPE (1, (SF, SF))
DEF_MIPS_FTYPE (2, (SF, SF, SF))
DEF_MIPS_FTYPE (1, (SF, V2SF))

DEF_MIPS_FTYPE (2, (SI, DI, SI))
DEF_MIPS_FTYPE (2, (SI, POINTER, SI))
DEF_MIPS_FTYPE (1, (SI, SI))
DEF_MIPS_FTYPE (2, (SI, SI, SI))
DEF_MIPS_FTYPE (3, (SI, SI, SI, SI))
DEF_MIPS_FTYPE (1, (SI, V2HI))
DEF_MIPS_FTYPE (2, (SI, V2HI, V2HI))
DEF_MIPS_FTYPE (1, (SI, V4QI))
DEF_MIPS_FTYPE (2, (SI, V4QI, V4QI))
DEF_MIPS_FTYPE (1, (SI, VOID))

DEF_MIPS_FTYPE (2, (UDI, UDI, UDI))
DEF_MIPS_FTYPE (2, (UDI, UV2SI, UV2SI))

DEF_MIPS_FTYPE (1, (USI, VOID))

DEF_MIPS_FTYPE (2, (UV2SI, UV2SI, UQI))
DEF_MIPS_FTYPE (2, (UV2SI, UV2SI, UV2SI))

DEF_MIPS_FTYPE (2, (UV4HI, UV4HI, UQI))
DEF_MIPS_FTYPE (2, (UV4HI, UV4HI, USI))
DEF_MIPS_FTYPE (2, (UV4HI, UV4HI, UV4HI))
DEF_MIPS_FTYPE (3, (UV4HI, UV4HI, UV4HI, UQI))
DEF_MIPS_FTYPE (3, (UV4HI, UV4HI, UV4HI, USI))
DEF_MIPS_FTYPE (1, (UV4HI, UV8QI))
DEF_MIPS_FTYPE (2, (UV4HI, UV8QI, UV8QI))

DEF_MIPS_FTYPE (2, (UV8QI, UV4HI, UV4HI))
DEF_MIPS_FTYPE (1, (UV8QI, UV8QI))
DEF_MIPS_FTYPE (2, (UV8QI, UV8QI, UV8QI))

DEF_MIPS_FTYPE (1, (V2HI, SI))
DEF_MIPS_FTYPE (2, (V2HI, SI, SI))
DEF_MIPS_FTYPE (3, (V2HI, SI, SI, SI))
DEF_MIPS_FTYPE (1, (V2HI, V2HI))
DEF_MIPS_FTYPE (2, (V2HI, V2HI, SI))
DEF_MIPS_FTYPE (2, (V2HI, V2HI, V2HI))
DEF_MIPS_FTYPE (1, (V2HI, V4QI))
DEF_MIPS_FTYPE (2, (V2HI, V4QI, V2HI))

DEF_MIPS_FTYPE (2, (V2SF, SF, SF))
DEF_MIPS_FTYPE (1, (V2SF, V2SF))
DEF_MIPS_FTYPE (2, (V2SF, V2SF, V2SF))
DEF_MIPS_FTYPE (3, (V2SF, V2SF, V2SF, INT))
DEF_MIPS_FTYPE (4, (V2SF, V2SF, V2SF, V2SF, V2SF))

DEF_MIPS_FTYPE (2, (V2SI, V2SI, UQI))
DEF_MIPS_FTYPE (2, (V2SI, V2SI, V2SI))
DEF_MIPS_FTYPE (2, (V2SI, V4HI, V4HI))

DEF_MIPS_FTYPE (2, (V4HI, V2SI, V2SI))
DEF_MIPS_FTYPE (2, (V4HI, V4HI, UQI))
DEF_MIPS_FTYPE (2, (V4HI, V4HI, USI))
DEF_MIPS_FTYPE (2, (V4HI, V4HI, V4HI))
DEF_MIPS_FTYPE (3, (V4HI, V4HI, V4HI, UQI))
DEF_MIPS_FTYPE (3, (V4HI, V4HI, V4HI, USI))

DEF_MIPS_FTYPE (1, (V4QI, SI))
DEF_MIPS_FTYPE (2, (V4QI, V2HI, V2HI))
DEF_MIPS_FTYPE (1, (V4QI, V4QI))
DEF_MIPS_FTYPE (2, (V4QI, V4QI, SI))
DEF_MIPS_FTYPE (2, (V4QI, V4QI, V4QI))

DEF_MIPS_FTYPE (2, (V8QI, V4HI, V4HI))
DEF_MIPS_FTYPE (1, (V8QI, V8QI))
DEF_MIPS_FTYPE (2, (V8QI, V8QI, V8QI))

DEF_MIPS_FTYPE (2, (VOID, SI, CVPOINTER))
DEF_MIPS_FTYPE (2, (VOID, SI, SI))
DEF_MIPS_FTYPE (1, (VOID, USI))
DEF_MIPS_FTYPE (2, (VOID, V2HI, V2HI))
DEF_MIPS_FTYPE (2, (VOID, V4QI, V4QI))
