/*******************************************************************************
*
* University of Illinois/NCSA
* Open Source License
*
* Copyright (c) 2018 Advanced Micro Devices, Inc. All Rights Reserved.
*
* Permission is hereby granted, free of charge, to any person obtaining a copy
* of this software and associated documentation files (the "Software"), to deal
* with the Software without restriction, including without limitation the
* rights to use, copy, modify, merge, publish, distribute, sublicense, and/or
* sell copies of the Software, and to permit persons to whom the Software is
* furnished to do so, subject to the following conditions:
*
*     * Redistributions of source code must retain the above copyright notice,
*       this list of conditions and the following disclaimers.
*
*     * Redistributions in binary form must reproduce the above copyright
*       notice, this list of conditions and the following disclaimers in the
*       documentation and/or other materials provided with the distribution.
*
*     * Neither the names of Advanced Micro Devices, Inc. nor the names of its
*       contributors may be used to endorse or promote products derived from
*       this Software without specific prior written permission.
*
* THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
* IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
* FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
* CONTRIBUTORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
* LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
* OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS WITH
* THE SOFTWARE.
*
*******************************************************************************/

#if !(defined HANDLE_ISA)
#error "Missing macro definition of HANDLE_ISA"
#endif

/*
* HANDLE_ISA(NAME, TRAP_HANDLER_ENABLED, LOCAL_MEMORY_SIZE, EUS_PER_CU,
*            MAX_WAVES_PER_CU, MAX_FLAT_WORK_GROUP_SIZE,
*            SGPR_ALLOC_GRANULE, TOTAL_NUM_SGPRS, ADDRESSABLE_NUM_SGPRS,
*            VGPR_ALLOC_GRANULE, TOTAL_NUM_VGPRS, ADDRESSABLE_NUM_VGPRS,
*            LDS_BANK_COUNT)
*/

HANDLE_ISA("amdgcn-amd-amdhsa--gfx700", false, 65536, 4, 40, 2048, 8, 512, 104, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx701", false, 65536, 4, 40, 2048, 8, 512, 104, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx702", false, 65536, 4, 40, 2048, 8, 512, 104, 4, 256, 256, 16)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx801+xnack", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx802", false, 65536, 4, 40, 2048, 16, 800, 96, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx803", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx810+xnack", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 16)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx900", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx900+xnack", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx902+xnack", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx904", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx906", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx906+sram-ecc", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx908", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx908+sram-ecc", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx909+xnack", false, 65536, 4, 40, 2048, 16, 800, 102, 4, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx1010", false, 65536, 4, 40, 2048, 106, 800, 106, 8, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx1011", false, 65536, 4, 40, 2048, 106, 800, 106, 8, 256, 256, 32)
HANDLE_ISA("amdgcn-amd-amdhsa--gfx1012", false, 65536, 4, 40, 2048, 106, 800, 106, 8, 256, 256, 32)

#undef HANDLE_ISA
